|  |  |
| --- | --- |
| KBWC-16K Wall Mount AC Motor Fan Speed Control | **KBWC-16K Wall Mount AC Motor Fan Speed Control** KBWC-16K 25°C Pkg. C, Part No. H9001The KBWC-16K is a Distributor packaged Solid State AC Motor Speed Fan Control. It is designed for mounting in a 2" X 4" electrical wall box. It operates from 115 VAC, 50/60 Hz and has a **maximum rating of 6.0 Amps @ 25°C**. The KBWC-16K provides infinitely variable speed motor control for Shaded Pole, Permanent Split Capacitor and Universal (AC/DC) motors. The variable speed motor control contains an on/off line switch, a high gain RFI noise suppres-sion filter, a minimum speed trimpot and a flame retardant ABS enclosure. Applications include range hoods, vibrators, humidifiers, fireplace blowers, fans, laminar flow hoods, heat tunnels and stirrers. See data sheet D-160 for optional features. The "K" suffix indicates, mounting kit that includes individual packaging with dial plate, knob, mounting screws, wire connectors and instructions. |

|  |  |
| --- | --- |
| KBWC-18K AC Motor Speed Fan Control | **KBWC-18K AC Motor Speed Fan Control**KBWC-18K 40°C Pkg. D, Part No. H9011The KBWC-18K is a Distributor packaged Solid State AC Motor Speed Fan Control. It is designed for mounting in a 2" X 4" electrical wall box. It operates from 115 VAC, 50/60 Hz and has a **maximum rating of 8.0 Amps @ 40°C**. The KBWC-18K provides infinitely variable speed motor control for Shaded Pole, Permanent Split Capacitor and Universal (AC/DC) motors. The variable speed motor control contains an on/off line switch, a high gain RFI noise suppres-sion filter, a minimum speed trimpot and a flame retardant ABS enclosure. Applications include range hoods, vibrators, humidifiers, fireplace blowers, fans, laminar flow hoods, heat tunnels and stirrers. See data sheet D-160 for optional features. The "K" suffix indicates, mounting kit that includes individual packaging with dial plate, knob, mounting screws, wire connectors and instructions. |